hostname SORU1

!

enable secret 5 $1$mERr$juIuYI4xUSJBYpeYD99wu.

!

ip dhcp pool SINAV

network 192.168.1.0 255.255.255.0

default-router 192.168.1.1

dns-server 8.8.8.8

!

interface FastEthernet0/0

ip address 192.168.1.1 255.255.255.0

ip nat inside

duplex auto

speed auto

!

interface FastEthernet0/1

ip address 192.168.2.1 255.255.255.0

ip nat inside

duplex auto

speed auto

!

interface Serial0/0

ip address 50.60.70.1 255.0.0.0

ip nat outside

!

interface FastEthernet1/0

ip address 192.168.0.1 255.255.255.0

ip nat inside

duplex auto

speed auto

!

router rip

network 50.0.0.0

network 192.168.0.0

network 192.168.1.0

network 192.168.2.0

!

ip nat pool GENEL 68.110.74.95 68.110.74.96 netmask 255.255.255.0

ip nat inside source list NAT pool GENEL overload

ip nat inside source static 192.168.0.100 68.110.74.100

ip classless

!

ip access-list standard NAT

deny 192.168.2.0 0.0.0.255

permit 192.168.0.0 0.0.255.255

line con 0

password ebg

login

!

line aux 0

!

line vty 0 4

password ebg

login

!

End

